|  |  |
| --- | --- |
|  | **Contact**Kathrin FleuchausMarketing CommunicationsCoperion GmbHTheodorstraße 1070469 Stuttgart/DeutschlandTelefon +49 (0)711 897 25 07kathrin.fleuchaus@coperion.comwww.coperion.com |
|  |
|  |
|  |

Press Release – Success Story

Coperion Compounding Technology for Current and Future Plastics Production Challenges

**Compounder** **Chuanghe Expands Production with Ten Coperion Twin Screw Extruders**

*Stuttgart, October 2023* – Chinese compounder Chuanghe new material technology Jiangsu Co., Ltd. is relying on the performance, reliability, and flexibility of Coperion extrusion systems for the expansion of its production capacity. This specialist in high-quality engineering plastics contracted with Coperion for ten STS Mc11 and ZSK Mc18 twin screw extruders. Most of these machines are already successfully in operation at the Chuanghe site in Yangzhou City, Jiangsu Province, PR China.

Chuanghe new material technology Jiangsu manufactures high-quality plastics for the automotive, household and electronics industries. Their products include various glass fiber reinforced engineering plastics as well as biodegradable plastics and even carbon-neutral produced plastics. The ten new compounding machines procured from long-established machine and plant specialist Coperion, headquartered in Germany, precisely fulfill the high demands that manufacturing such plastics places on production technology.

**High-performance Coperion compounder for the greatest flexibility and reliability**

Chuanghe is expanding its production with several compounding machines from Coperion in order to be able to act with greater flexibility in both small batch production as well as large quantity manufacturing. For this reason, Chuanghe has invested in six Coperion STS Mc11 twin screw extruders of various sizes – from the STS 25 Mc11 laboratory extruder with a 25 mm screw diameter to the STS 75 Mc11 with a diameter of 75 mm.

Moreover, Chuanghe has acquired four high-performance extruders from the Coperion ZSK series – two ZSK 58 Mc18 models with 58 mm screw diameter for PA throughputs of up to 800 kg/h as well as two ZSK 70 Mc18 with 70 mm screw diameter for PA throughputs up to 1,600 kg/h – specifically for large-batch manufacturing of demanding engineering plastics. These four ZSK Mc18 extruders stand out for their especially high specific torque of 18 Nm/cm³. Due to the material’s short residence time in the extruder, these machines operate extremely gently, achieving consistently high product quality. They are each equipped with ZS-B side feeders so that Chuanghe can exercise tremendous flexibility in compounding its plastics using various additives. All volatile components released from the plastic during production are securely degassed from the process using ZS-EG side degassing units – yet another indicator of reliable, first-class product quality.

**Visionary production expansion that promises success**

This expansion of its machinery optimally positions Chuanghe new material technology Jiangsu for future market demands. Thanks to constant process parameters across the entire model series, Coperion extruders allow for secure scale-up from one extruder size to another, which in this case gives Chuanghe complete flexibly to utilize its machinery to full capacity. Moreover, Coperion extruders’ modular design and numerous quick change features provide the flexibility necessary to implement quick recipe changes. At the same time, Coperion extruders possess the necessary prerequisites to be able to master future tasks in plastics compounding.

Joanne Shen, Managing Director of Coperion Nanjing, is very pleased: “We’re excited by the close working relationship with Chuanghe new material technology Jiangsu and we are gratified by the trust that Chuanghe has placed in us with this major order. We are proud to see how the installed machines are already demonstrating their high performance, reliability, and flexibility on a daily basis. We are certain that Chuanghe has paved the way for meeting future challenges with this expansion of their production capabilities. As a technology partner with comprehensive process expertise, we will continue to stand at Chuanghe’s side to support them closely along the way.”

**About Coperion**

Coperion ([www.coperion.com](http://www.coperion.com)) is a global industry and technology leader in compounding and extrusion systems, sorting, size reduction and washing systems, feeding systems, bulk material handling and services. Coperion develops, produces, and services plants, machinery, and components for the plastics and plastics recycling industry as well as the chemical, batteries, food, pharmaceutical and minerals industries. Coperion employs 4,000 people in its three divisions, Polymer, Food, Health & Nutrition, and Aftermarket Sales & Service, and in its 40 sales and service companies worldwide. Coperion is an Operating Company of Hillenbrand (NYSE: HI), a global industrial company that provides highly-engineered, mission-critical processing equipment and solutions to customers serving a wide variety of industries around the world. [www.hillenbrand.com](http://www.hillenbrand.com)

**About Chuanghe new material technology Jiangsu**Chuanghe new material technology Jiangsu Co., Ltd. is a comprehensive new material enterprise that integrates scientific research, production, sales and service, providing a new complete material solution for creating a more friendly, comfortable and healthy human life. The technical team has more than 20 years of experience in the research and development, production and sales of modified plastics, and the core technology is completely independently developed. On this basis, Chuanghe carries out in-depth cooperation with the majority of relevant colleages and social professional teams. Specializing in the field of new material modified general plastics, modified engineering plastics, special engineering plastics, biodegradable materials and other polymer materials of high-tech enterprises. Mainly used in rail transit, energy storage, power tools, smart home, household appliances, new energy vehicles, electronic communications and medical supplies and other fields.



Dear colleagues,
You will find this press release in English and Chinese together with the pictures in printable quality for download at

[**https://www.coperion.com/en/news-media/newsroom/**](https://www.coperion.com/en/news-media/newsroom/)

 .

Editor contact and copies:

Dr. Jörg Wolters, KONSENS Public Relations GmbH & Co. KG,
Hans-Böckler-Str. 20, D - 63811 Stockstadt am Main
Tel.: +49 (0)60 27/99 00 5-0
E-mail: mail@konsens.de, Internet: www.konsens.de

Coperion twin screw extruders stand out for their especially high output, reliability, and flexibility in compounding plastics.

*Photo: Coperion, Stuttgart Germany*

Chuanghe has acquired four of Coperion’s high-performance ZSK Mc18 twin screw extruders.

*Photo: Chuanghe new material technology, PR China*