|  |  |
| --- | --- |
| Coperion GmbH, 70466 Stuttgart, Germany | Coperion GmbHTheodorstrasse 1070469 Stuttgart, GermanyTelefax +49 711 897 3976repair@coperion.comwww.coperion.com |
|  |
| **Return Material Authorization (Die Plate)****Originator / Billing address: (Please complete all lines)** |
| **Customer no.:** |       |  |
| **Company:** |       |  |
| **Contact person:** |       |  |
| **Department:** |       |  |
| **Street:** |       |  |
| **Postal Code:** |       | **City:** |       |  |
| **Phone:** |       | **Fax:** |       |  |
| **E-Mail address:** |       | @ |       |
|  |
| **CustomerOrder no.:** |       |
| **Items belong to:** |       |
| Machine: |       |
| Machine size: |       |
| Machine no. / Project no. / Work no.: |       |
|  |
| **Die Plate Size** | **Serial No.**(4-digit no. on outer circumference) | **Operating hours** | **Reason for return (1)** | **Required spare parts (2)** |
|       |       |       |       |       |
|       |       |       |       |       |
|       |       |       |       |       |
| **Reason for return (1)** | **Required spare parts (2)** |
| A | Regrinding after operating period |  | 1 | None |
| B | Defective (transport damage) |  | 2 | Sealing and insulation material |
| C | Warranty claim |  | 3 | Metal cover plate and disk, including screws |
| D | Error analysis\* |  | 4 | Set of screws for mounting on die head |
| E | Other\*\*  |  |  |  |
|  |  |  |  |
| \*For all inspection reports we need a detailed description of the problem.\*\*Please describe in separate letter |
| **Return Material Authorization (Die Plate)**For deliveries outside the EU we need additional information about the value of goods for thecustoms and the HS code! Without this information, export after repair is not possible.**Price list for die plate refurbishments (01/2021)**

|  |  |
| --- | --- |
| **Die plate size** | **Price** |
| UG 400 | 6.800 EUR |
| UG 500, 525, 550 | 7.400 EUR |
| UG 700, 725, 750 | 8.600 EUR |
| UG 925, 1000 | 10.100 EUR |
| UG 1250 | 12.100 EUR |

**Including:**Cleaning, CMM, Pressure Test, Check all threads, Appraisal, Grinding (back and front), CMM, Die Penetrant test, Pressure test, Final Inspection, Prep for Shipment, ConservationThe refurbishment does not contain any special procedures or accessory spare parts.if we face a higher repair efforts compared to our standard procedure we reserve a price adjustment.With a return shipment you agree to cover these costs for cleaning and investigation of the necessary repair steps.Before we start a repair you will receive a preliminary cost estimate for approval.Please make sure that the return shipment will be delivered under incoterm DDP. Please indicate the real present amount of the part in the customs invoice!Please notice, that we cannot create a Certificate of Origin (COO) for repairs.Please attach a copy to the return shipment.**Declaration:** (confirmation by checkmark click necessary)[ ]  The component has been carefully cleaned and is free of harmful adhesions. There are no risks.[ ]  The following residual hazard exists or could not be eliminated, the following characteristic hazard characteristics according to the GHS regulation may still exist:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
| GHS 01 | GHS 02 | GHS 03 | GHS 04 | GHS 05 |
| [ ] **GHS01** | [ ] **GHS02** | [ ] **GHS03** | [ ] **GHS04** | [ ] **GHS05** |
| GHS 06 | GHS 07 | GHS 08 | GHS 09 |  |
| [ ] **GHS06** | [ ] **GHS07** | [ ] **GHS08** | [ ] **GHS09** |  |

* **If one of these hazard characteristics is ticked, the corresponding current EU safety data sheet in German must also be sent in.**
* **Without the corresponding information we are unfortunately unable to execute your order.**

**Important!*** Whenever a customer is sending us material, i.e. for refurbishment -and/or repair works or further specific reason, it is **mandatory**, to send us the RMA sheet, filled out with all requested data. One sheet should be sent **before** dispatch to our email we-coperion@era.de and one sheet should **always inside the box**, accompanied with the goods. This will help us, to identify the material quickly and avoid further clarification. The RMA can be downloaded through our homepage.
* Material which will be sent without RMA sheet will be not accepted from Coperion anymore. Please note, that additional costs like transport, storage or any further kind of fees will be charged directly to the customer.
* Please support us in this regard in order to assure a smooth procedure.

**Return Material Authorization (Die Plate)**Address for return delivery to our die plate workshops: |
| **Coperion Germany** | **Coperion Middle East** | **Coperion USA** |
| Coperion GmbHc/o ERA Spedition GmbHFriedenstraße 6-1070806 KornwestheimGermanyOpening hours of the incoming goods department **Stuttgart** 7 a.m. to 3:00 p.m.- Your contact person for notifications can be reached via the following email address:we-coperion@era.de | Coperion Middle East Co. Ltd.Street # 327, Sector G, Block 2,LOT # 31Jubail 2 Industrial City 31961Saudi-Arabia | Coperion Corporation196 Applachian DriveWytheville VA 24382United States of America |
| Date: |       |  |
|  |
| Name: |       |  |
|  |
| Signature: |  |  |
|  |
|  |
|  |
| Your company stamp |
|  |
|  |